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Important Product Info

The surface of all Postal Products Manufacturing clear aluminum or powder coated products may be cleaned of dirt or grime with a soft cloth dampened with any mild detergent or properly diluted biodegradable, water-based cleaner, such as “Simple Green™”.  Wipe from top to bottom avoid run-down.  Avoid use of abrasives, which might damage the product surface.  Rinse with plain water and dry.  Avoid cleaning during extreme temperature conditions. 

[image: Image result for postal products unlimited 4c]To varying extents, depending upon the color, it may be possible to remove some spray-paint or marker-applied graffiti from powder coated surfaces by using a stronger cleaner such as “Krud Kutter™” or a mild petroleum-based solvent, such as mineral spirits.  Test-clean a small area first, a few seconds at a time.  Do not allow chemical to remain on surface for an indefinite period, as this may damage the surface of the product.  Remove any residue left with a mild cleaner, followed by water rinse as noted above. 

Matching touch-up paint products may be available from an Authorized Postal Products Dealer for products which utilize powder coat finishes.

If a mailbox lock in outdoor equipment becomes clogged with ice due to extreme winter conditions, the lock manufacture suggest using “Tri-Flow® Superior Lubricant Aerosol”.  Spray the Tri-Flow® Lubricant directly into the keyhole and onto the key.  Slide the key in and out of the lock several times to spread the lubricant.  Do not apply much product, as a small amount is sufficient.  Wipe off any excess lubricant from the lock and key. 
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